Fusion 23.2.0 Connect Help Center

# Media Server connection

You can use your existing OpenText IDOL Media Server implementation to perform optical character recognition (OCR) on documents managed by Fusion.

Fusion includes a default OCR configuration file that defines a Media Server analysis task for basic OCR and uses a custom XSL to manipulate the Media Server response to only that which Fusion requires. This configuration does not apply orientation correction, cropping, or template or region detection. You can create custom Media Server configurations to perform OCR analysis tasks.

If you plan to connect to Media Server to facilitate optical character recognition (OCR), additional tasks are required

## Requirements

Prior to beginning the connection tasks, you must have the following in place.

- Fusion processing agent fully installed and configured, following practices and procedures defined in Agent installation and configuration.

  NOTE: Each processing agent host can connect to a single Media Server host.

- Supported version of Media Server fully installed and configured, following standard Media Server practices and procedures. For supported version of Media Server, see Support matrix > Integrated Resources.

- Fusion agents and any Media Server host machines they interact with must be within the same network and can not have a proxy between them.

- Ensure the Media Server host machine IP or server name is resolvable to the Fusion processing agent host machine it will be connected to.

- If you plan to use existing or new Media Server configurations to perform OCR analysis tasks, ensure that these configurations have been verified and tested in Media Server and conform to the necessary format for compatibility with Fusion. For configuration format information, see Custom Media Server configurations for OCR task analysis.

## Update Media Server

You must update your Media Server implementation to include the necessary components to interact with Fusion

To update Media Server for OCR through Fusion

1. On a Media Server host machine that will be connected to a processing agent host, ensure the necessary parameters and values are present in the Media Server configuration file, `mediaserver.cfg`.

   - Under `[Paths]`, verify the following parameters and values are present. If not present, add them.

     - `LuaDirectory=configurations/lua`

     - `XslDirectory=configurations/xsl`

     - `TemplateDirectory=configurations/xsl/response_templates`

   - Under `[Modules]`, verify the `Enable` parameter includes the `ocr` and `objectrecognition` modules in the list of values.

   - Under `[Channels]`, verify at least one at least one channel of type Visual is enabled.

     Example: `VisualChannels=1`

2. Copy the required files from the Fusion processing agent host machine to the Media Server host machine.

   - From the installation path for the Fusion processing agent, copy `getMediaBoundary.lua` from the `mediaserver/lua` directory to the `/configurations/lua` directory in the installation path for Media Server.

   - From the installation path for the Fusion processing agent, copy all files from the `/mediaserver/xsl` directory to the `/configurations/xsl` directory in the installation path for Media Server.

3. Restart the Media Server service.

4. Repeat for each Media Server host that will be connected to a processing agent host for OCR.

## Update Fusion

You must update your Fusion processing agent implementation to include the necessary components to use Media Server for OCR.

To update Fusion for OCR using Media Server

1. Update Media Server connection information in the agent Administration UI.

   1. On the agent host server that will connect to a Media Server host, open the agent Administration UI.

      From the Start menu, click Fusion Agent > Agent Admin.

      The UI opens to System Status.

   2. In the primary navigation panel, click Advanced Settings.

   3. In the Category list on the Advanced Settings page, click Analyze.

   4. Complete the following options for the Media Server you want to connect to.

      Option | Description
      --- | ---
      Media Server Host | Type the IP address or fully qualified domain name of the Media Server host that this agent will connect to. Defaults to `localhost`.
      Media Server Port | Verify the port number for the Media Server host that this agent will connect to. Defaults to `14000`. This is the default port for Media Server.
      Media Server Configuration Directory | Verify the relative path to the directory on this agent server host to the Media Server configuration files. Defaults to `[Common\Base Path]\Config`, where `[Common\Base Path]` is the agent installation path on this agent host. The Base Path can be seen on this page. OCR configuration files for Media Server analysis tasks must be in this directory. CAUTION: Do not change this unless you moved the directory where the Media Server configuration files for OCR analysis tasks are placed on this agent host. You can create a subfolder if desired; the subfolder would then be considered the new root when defining configuration files when creating a dataset.
      Media Server Default Configuration File Name | Verify the name of the default Media Server configuration file for OCR analysis tasks. Defaults to `OCR_Only.cfg`. CAUTION: Do not change this unless you have placed a valid alternate configuration file in the directory defined by the Media Server Configuration Directory. If you have alternate configuration files, see Custom Media Server configurations for OCR task analysis.
      Media Server Set Https | Verify this matches your Media Server implementation. Set to `True` only if your Media Server is set to use Https. Defaults to `False`.

2. If applicable, copy any custom Media Server configuration files for OCR analysis tasks to the agent host.

   Place the configuration files in the path defined by the Media Server Configuration Directory. By default this is `C:\Program Files\Micro Focus\FAS\Agent\Config`.

3. Repeat for each processing agent host that will connect to a Media Server host to perform OCR.

## Custom Media Server configurations for OCR task analysis

If you choose to create your own Media Server configurations for OCR task analysis, follow all procedures, guidelines, and suggestions for OCR as documented in the Media Server documentation. The Media Server Administration Guide contains the necessary details and includes information for improving OCR and optimizing performance for object recognition.

Fusion expects a response engine type to facilitate the processing of the extracted metadata. The response engine must have the following format:

    [ResponseEngineName]
    Type = response
    Input = OCREngineName.Result

Example response

    [Response]
    Type = response
    Input = OCR.Result

If defining regions for OCR, you can use Media Server Visual Training to develop a template. A template consists of a series of regions which contain a name and set of region coordinates (in pixels). Each region defined in Media Server must have two respective engines in the processing configuration: a `SetRectangle` type engine and an `ocr` type engine. It is not a requirement for either engine to be named exactly the same as the respective Media Server metadata field, though there is a naming convention for the `ocr` type engine that must be followed to work correctly with the Fusion agent. During document ingestion,Fusion uses the name of each `ocr` type engine to define the respective value leveraged.

The format of the `ocr` engine type region name must use the format `<OBJECT_TYPE>-<REGION_NAME>-<REGION_TYPE>`. The `<OBJECT_TYPE>-` must always exist and come first. There must be a separating hyphen '-' between each portion with a minimum of one (`<OBJECT_TYPE>-<REGION_TYPE>`) and maximum of two (`<OBJECT_TYPE>-<REGION_NAME>-<REGION_TYPE>`).

Example region-based OCR configuration file compatible for Fusion (English)

    [Session]
    Engine0 = Source
    Engine1 = DetectAnchor
    Engine2 = RotateIdCard
    Engine3 = IdCardRegion
    Engine4 = CropIdCard

    # Drivers License fields
    Engine5 = DriversLicense-TextRegion_Address
    Engine6 = DriversLicense-Address
    Engine7 = DriversLicense-TextRegion_Forename
    Engine8 = DriversLicense-Forename
    Engine9 = DriversLicense-TextRegion_Surname
    Engine10 = DriversLicense-Surname

    Engine11 = CombineResultsWithSources

    Engine12 = Response

    #
    # Ingest
    #
    [Source]
    Type = image

    #
    # Analysis
    #
    [DetectAnchor]
    Type = ObjectRecognition
    Database = IDCardTemplates
    Geometry = SIM2

    #
    # Transform
    #
    [RotateIdCard]
    Type = Rotate
    Input = DetectAnchor.ResultWithSource
    LuaLine = function getAngle(x) return -x.ObjectRecognitionResultAndImage.inPlaneRotation end

    [IdCardRegion]
    Type = SetRectangle
    Input = DrawOnIdCard.Output
    LuaScript = getMediaBoundary.lua

    [CropIdCard]
    Type = Crop
    Input = IdCardRegion.Output

    #
    # Drivers License - OCR by region
    #
    [DriversLicense-TextRegion_Address]
    Type = SetRectangle
    Input = DetectCroppedImageAnchor.ResultWithSource
    LuaScript = getTurkey_DriverLicense_OCR_Address.lua

    [DriversLicense-Address]
    Type = ocr
    OCRMode = document
    Input = DriversLicense-TextRegion_Address.Output
    RestrictToInputRegion = true
    Languages = tr
    CharacterTypes = alpha,digit

    [DriversLicense-TextRegion_Forename]
    Type = SetRectangle
    Input = DetectCroppedImageAnchor.ResultWithSource
    LuaScript = getTurkey_DriverLicense_OCR_Forename.lua

    [DriversLicense-Forename]
    Type = ocr
    OCRMode = document
    Input = DriversLicense-TextRegion_Forename.Output
    RestrictToInputRegion = true
    Languages = tr
    CharacterTypes = alpha

    [DriversLicense-TextRegion_Surname]
    Type = SetRectangle
    Input = DetectCroppedImageAnchor.ResultWithSource
    LuaScript = getTurkey_DriverLicense_OCR_Surname.lua

    [DriversLicense-Surname]
    Type = ocr
    OCRMode = document
    Input = DriversLicense-TextRegion_Surname.Output
    RestrictToInputRegion = true
    Languages = tr
    CharacterTypes = uppercase

    #
    # Event Processing
    #
    [CombineResultsWithSources]
    Type=or
    Input0 = DriversLicense-Address.ResultWithSource
    Input1 = DriversLicense-Forename.ResultWithSource
    Input2 = DriversLicense-Surname.ResultWithSource

    [Response]
    Type=response
    Input=CombineResultsWithSources.Output

Additional engine types, such as `passport`, can be added as desired. Ensure engine names are unique and use sequential ordering where appropriate.

For grammar value extraction using a template or region-based configuration and metadata fields within OCR results need to be in a language context other than English, the `ocr` engines need to be URL encoded throughout the configuration file. As an example, a Turkish driver's license includes "Sürücü belgesi", which translates to "driver's license" in English. The engine type must be declared with the non-English characters in "Sürücü" URL encoded as follows:

    Engine12 = DriversLicense-S%C3%BCr%C3%BCc%C3%BC_belgesi

Example `ocr` engine type configuration sections with URL encoding for Turkish driver's license

`ocr` type engine definition section

    [DriversLicense-S%C3%BCr%C3%BCc%C3%BC_belgesi]
    Type = ocr
    OCRMode = document
    Input = DriversLicense-TextRegion_Code5.Output
    RestrictToInputRegion = true
    Languages = tr
    CharacterTypes = digit

`ocr` type engine usage section for event processing results

    [CombineResultsWithSources]
    Type=or
    Input0 = DriversLicense-Address.ResultWithSource
    Input1 = DriversLicense-Code4d.ResultWithSource
    Input2 = DriversLicense-S%C3%BCr%C3%BCc%C3%BC_belgesi.ResultWithSource
    Input3 = DriversLicense-Date_Of_Birth.ResultWithSource

The LuaScript file of the `SetRectangle` type engine includes the actual name of the respective Media Server metadata field that is used and therefore serves as the mapping between the configuration and the Media Server metadata region field. The region's coordinates defined in Media Server are used to get the region rectangle on the on-the-fly cropped image and the subsequent `ocr` engine uses this to OCR scan only the contents of that region.

If fields in the layout of the card/template/image are generally required to be together as one field for successful grammar value extraction, such as forename and surname, you can group these fields. Within the configuration, group these fields together into a single field (`or` type engine) and use the group output as a single entry input used for the Media Server response.

Example configuration for grouped fields for OCR

    # Drivers License fields
    Engine19 = DriversLicense-TextRegion_Forename
    Engine20 = DriversLicense-Forename
    Engine21 = DriversLicense-TextRegion_IssueDate
    Engine22 = DriversLicense-Issue_Date
    Engine23 = DriversLicense-TextRegion_Surname
    Engine24 = DriversLicense-Surname

    # National Id fields
    Engine29 = NationalId-TextRegion_Forename
    Engine30 = NationalId-Forename
    Engine31 = NationalId-TextRegion_Surname
    Engine32 = NationalId-Surname

    # Drivers License sub-groups (combines)
    Engine43 = DriversLicense-Name

    # National Id  sub-groups (combines)
    Engine44 = NationalId-Name

    [DriversLicense-Name]
    Type=or
    Input0 = DriversLicense-Forename.ResultWithSource
    Input1 = DriversLicense-Surname.ResultWithSource

    [NationalId-Name]
    Type=or
    Input0 = NationalId-Forename.ResultWithSource
    Input1 = NationalId-Surname.ResultWithSource

    [CombineResultsWithSources]
    Type=or
    Input0 = DriversLicense-Address.ResultWithSource
    Input1 = DriversLicense-Code4d.ResultWithSource
    Input2 = DriversLicense-S%C3%BCr%C3%BCc%C3%BC_belgesi.ResultWithSource
    Input3 = DriversLicense-Date_Of_Birth.ResultWithSource
    Input4 = DriversLicense-Place_Of_Birth.ResultWithSource
    Input5 = DriversLicense-Expiry_Date.ResultWithSource
    Input6 = DriversLicense-Name.Output
    Input7 = DriversLicense-Issue_Date.ResultWithSource
    Input8 = DriversLicense-Vehicle_Types.ResultWithSource
    Input9 = NationalId-Identity_No.ResultWithSource
    Input10 = NationalId-Name.Output
    Input11 = NationalId-Date_Of_Birth.ResultWithSource
    Input12 = NationalId-Gender.ResultWithSource
    Input13 = NationalId-Document_No.ResultWithSource
    Input14 = NationalId-Nationality.ResultWithSource
    Input15 = NationalId-Valid_Until.ResultWithSource

    [Response]
    Type=response
    Input=CombineResultsWithSources.Output

For the sub-grouping to be picked up and handled correctly, copy the updated `toAgentDataResponse.xsl` file on the agent host (`<agentInstallDir>\mediaserver\xsl\response_templates\toAgentDataResponse.xsl`) and paste in the `\response_templates` directory on each Media Server ‘host managed by this agent (`<MediaServerInstallDir>\ configurations\xsl\response_templates`), overwriting the existing file if necessary. It is within this XSL transform that the detected OCR text value for each item in a group is concatenated in the order specified in the respective group `or` type engine (input0, input1…inputN). An average confidence value for all the engine results in the group is also generated for the single record output.

For further guidance on custom Media Server configuration, contact Support.

Copyright 2019-2023 Open Text
Version 23.2.0 | Last updated May 2023
Connect
Marketplace
Learn
Support portal
Documentation
Contact
Submit or view service request