Controller 25.2
Controller Reference

# TTL

The Time To Live of multicast IP packets for SSDP (that is, how many router hops are allowed). This option determines the scope of the SSDP deployment in your network.

Type: | Integer
Default: | 2
Required: | No
Configuration Section: | SSDP
Example: | `TTL=2`
See Also: |

Copyright 2015-2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Controller 25.2

Topic Title: TTL